Package dns :: Package rdtypes :: Package ANY :: Module GPOS |
[hide private]
[frames] | no frames]

# Source Code for Module dns.rdtypes.ANY.GPOS

      1  # Copyright (C) 2003-2007, 2009, 2010 Nominum, Inc.
      2  #
      3  # Permission to use, copy, modify, and distribute this software and its
      4  # documentation for any purpose with or without fee is hereby granted,
      5  # provided that the above copyright notice and this permission notice
      6  # appear in all copies.
      7  #
      8  # THE SOFTWARE IS PROVIDED "AS IS" AND NOMINUM DISCLAIMS ALL WARRANTIES
      9  # WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
     10  # MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL NOMINUM BE LIABLE FOR
     11  # ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
     12  # WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
     13  # ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT
     14  # OF OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
     15
     16  import dns.exception
     17  import dns.rdata
     18  import dns.tokenizer
     19
     20 -def _validate_float_string(what):
     21      if what[0] == '-' or what[0] == '+':
     22          what = what[1:]
     23      if what.isdigit():
     24          return
     25      (left, right) = what.split('.')
     26      if left == '' and right == '':
     27          raise dns.exception.FormError
     28      if not left == '' and not left.isdigit():
     29          raise dns.exception.FormError
     30      if not right == '' and not right.isdigit():
     31          raise dns.exception.FormError
     32
     33 -class GPOS(dns.rdata.Rdata):
     34      """GPOS record
     35
     36      @ivar latitude: latitude
     37      @type latitude: string
     38      @ivar longitude: longitude
     39      @type longitude: string
     40      @ivar altitude: altitude
     41      @type altitude: string
     42      @see: RFC 1712"""
     43
     44      __slots__ = ['latitude', 'longitude', 'altitude']
     45
     46 -    def __init__(self, rdclass, rdtype, latitude, longitude, altitude):
     47          super(GPOS, self).__init__(rdclass, rdtype)
     48          if isinstance(latitude, float) or \
     49             isinstance(latitude, int) or \
     50             isinstance(latitude, long):
     51              latitude = str(latitude)
     52          if isinstance(longitude, float) or \
     53             isinstance(longitude, int) or \
     54             isinstance(longitude, long):
     55              longitude = str(longitude)
     56          if isinstance(altitude, float) or \
     57             isinstance(altitude, int) or \
     58             isinstance(altitude, long):
     59              altitude = str(altitude)
     60          _validate_float_string(latitude)
     61          _validate_float_string(longitude)
     62          _validate_float_string(altitude)
     63          self.latitude = latitude
     64          self.longitude = longitude
     65          self.altitude = altitude
     66
     67 -    def to_text(self, origin=None, relativize=True, **kw):
     68          return '%s %s %s' % (self.latitude, self.longitude, self.altitude)
     69
     70 -    def from_text(cls, rdclass, rdtype, tok, origin = None, relativize = True):
     71          latitude = tok.get_string()
     72          longitude = tok.get_string()
     73          altitude = tok.get_string()
     74          tok.get_eol()
     75          return cls(rdclass, rdtype, latitude, longitude, altitude)
     76
     77      from_text = classmethod(from_text)
     78
     79 -    def to_wire(self, file, compress = None, origin = None):
     80          l = len(self.latitude)
     81          assert l < 256
     82          byte = chr(l)
     83          file.write(byte)
     84          file.write(self.latitude)
     85          l = len(self.longitude)
     86          assert l < 256
     87          byte = chr(l)
     88          file.write(byte)
     89          file.write(self.longitude)
     90          l = len(self.altitude)
     91          assert l < 256
     92          byte = chr(l)
     93          file.write(byte)
     94          file.write(self.altitude)
     95
     96 -    def from_wire(cls, rdclass, rdtype, wire, current, rdlen, origin = None):
     97          l = ord(wire[current])
     98          current += 1
     99          rdlen -= 1
    100          if l > rdlen:
    101              raise dns.exception.FormError
    102          latitude = wire[current : current + l]
    103          current += l
    104          rdlen -= l
    105          l = ord(wire[current])
    106          current += 1
    107          rdlen -= 1
    108          if l > rdlen:
    109              raise dns.exception.FormError
    110          longitude = wire[current : current + l]
    111          current += l
    112          rdlen -= l
    113          l = ord(wire[current])
    114          current += 1
    115          rdlen -= 1
    116          if l != rdlen:
    117              raise dns.exception.FormError
    118          altitude = wire[current : current + l]
    119          return cls(rdclass, rdtype, latitude, longitude, altitude)
    120
    121      from_wire = classmethod(from_wire)
    122
    123 -    def _cmp(self, other):
    124          v = cmp(self.latitude, other.latitude)
    125          if v == 0:
    126              v = cmp(self.longitude, other.longitude)
    127              if v == 0:
    128                  v = cmp(self.altitude, other.altitude)
    129          return v
    130
    131 -    def _get_float_latitude(self):
    132          return float(self.latitude)
    133
    134 -    def _set_float_latitude(self, value):
    135          self.latitude = str(value)
    136
    137      float_latitude = property(_get_float_latitude, _set_float_latitude,
    138                                doc="latitude as a floating point value")
    139
    140 -    def _get_float_longitude(self):
    141          return float(self.longitude)
    142
    143 -    def _set_float_longitude(self, value):
    144          self.longitude = str(value)
    145
    146      float_longitude = property(_get_float_longitude, _set_float_longitude,
    147                                 doc="longitude as a floating point value")
    148
    149 -    def _get_float_altitude(self):
    150          return float(self.altitude)
    151
    152 -    def _set_float_altitude(self, value):
    153          self.altitude = str(value)
    154
    155      float_altitude = property(_get_float_altitude, _set_float_altitude,
    156                                doc="altitude as a floating point value")
    157